IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Projektnummer"
Time stamp: "2020-09-24T14:45:10"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (DEU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (DEU)"

People and organizations
  Person "christina.baartQ88XW" of Organization (no name given)
  Owner history of Person "christina.baartQ88XW" of Organization (no name given) | application "Autodesk Revit 2017 (DEU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 52° 30′ 59.765625″ | longitude 13° 23′ 59.998626″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Projektadresse", "Berlin", "Deutschland"
      IFCBUILDINGSTOREY "Ebene 0" | long name "Ebene 0" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basiswand:MW 24.0 WD 12.0" | object type "Basiswand:MW 24.0 WD 12.0:3900" | names: "Basiswand:MW 24.0 WD 12.0:388672" | material: layers "Basiswand:MW 24.0 WD 12.0" ("Wärmedämmung - hart" 0.12, "Mauerwerk - Ziegel, verputzt" 0.24) | property sets: Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "KNX Tastsens.3 Basis 1f Flächenschalter Reinweiß" | object type "KNX Tastsens.3 Basis 1f Flächenschalter Reinweiß" | names: "Gira_2021112:KNX Tastsens.3 Basis 1f Flächenschalter Reinweiß:452653" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation

Types
  IFCWALLTYPE "Basiswand:MW 24.0 WD 12.0" | STANDARD | 1 occurrence | material: layers "Basiswand:MW 24.0 WD 12.0" ("Wärmedämmung - hart" 0.12, "Mauerwerk - Ziegel, verputzt" 0.24)
  IFCBUILDINGELEMENTPROXYTYPE "KNX Tastsens.3 Basis 1f Flächenschalter Reinweiß" | 1 occurrence

Property sets
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "MW 24.0 WD 12.0" (IFCIDENTIFIER)
    ThermalTransmittance = 0.258196721311475 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "KNX Tastsens.3 Basis 1f Flächenschalter Reinweiß" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Gira" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)